ADDRESS_ACLR_B=NONE
ADDRESS_REG_B=CLOCK0
BYTE_SIZE=8
CLOCK_ENABLE_INPUT_A=BYPASS
CLOCK_ENABLE_INPUT_B=BYPASS
CLOCK_ENABLE_OUTPUT_B=BYPASS
INTENDED_DEVICE_FAMILY="Cyclone V"
LPM_TYPE=altsyncram
NUMWORDS_A=65536
NUMWORDS_B=65536
OPERATION_MODE=DUAL_PORT
OUTDATA_ACLR_B=NONE
OUTDATA_REG_B=CLOCK0
POWER_UP_UNINITIALIZED=FALSE
RDCONTROL_REG_B=CLOCK0
READ_DURING_WRITE_MODE_MIXED_PORTS=DONT_CARE
WIDTHAD_A=16
WIDTHAD_B=16
WIDTH_A=48
WIDTH_B=48
WIDTH_BYTEENA_A=6
DEVICE_FAMILY="Cyclone V"
address_a
address_b
byteena_a
clock0
data_a
rden_b
wren_a
q_b
